BNO:

VIN to 5V

GND to GND

SDA to 20

SCL to 21

Grayson code

Shield 13 to mega 52

SHIELD 12 TO MEGA 50

Shield 11 to mega 51

shield 10 to 53